;/*++
;
;Module Name:
;
;    SILABSER.INF
;
;    Copyright 2018, Silicon Laboratories Inc.
;
;Abstract:
;    Installation INF for Silicon Labs CP210x device
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Provider%
DriverVer = 05/07/2018,10.1.2.2115
CatalogFile = silabser.cat
PnpLockDown=1

; ================= Device section =====================

[Manufacturer]
%ManufacturerName%=SiLabsModelsSection, NTamd64.10, NTarm.10, NTarm64.10, NTx86.10

; "Architecture must be specified in INF Models sections names" -- meaning lots of
; cut'n'paste duplication in these next four per-Architecture ModelsSections
;Models section for installation of x64 driver on Windows 10 and above
[SiLabsModelsSection.NTamd64.10]
%USB\VID_10C4&PID_EA60.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA60
%USB\VID_10C4&PID_EA63.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA63
%USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_00
%USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_01
%USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_00
%USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_01
%USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_02
%USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_03
%USB\VID_10C4&PID_EA7A&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_00
%USB\VID_10C4&PID_EA7A&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_00
%USB\VID_10C4&PID_EA7B&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_02
%USB\VID_10C4&PID_EA7B&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_03

;Models section for installation of ARM (32-bit) driver on Windows 10 and above
[SiLabsModelsSection.NTarm.10]
%USB\VID_10C4&PID_EA60.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA60
%USB\VID_10C4&PID_EA63.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA63
%USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_00
%USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_01
%USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_00
%USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_01
%USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_02
%USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_03
%USB\VID_10C4&PID_EA7A&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_00
%USB\VID_10C4&PID_EA7A&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_00
%USB\VID_10C4&PID_EA7B&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_02
%USB\VID_10C4&PID_EA7B&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_03

;Models section for installation of ARM (64-bit) driver on Windows 10 and above
[SiLabsModelsSection.NTarm64.10]
%USB\VID_10C4&PID_EA60.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA60
%USB\VID_10C4&PID_EA63.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA63
%USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_00
%USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_01
%USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_00
%USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_01
%USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_02
%USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_03
%USB\VID_10C4&PID_EA7A&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_00
%USB\VID_10C4&PID_EA7A&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_00
%USB\VID_10C4&PID_EA7B&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_02
%USB\VID_10C4&PID_EA7B&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_03

;Models section for installation of x86 driver on Windows 10 and above
[SiLabsModelsSection.NTx86.10]
%USB\VID_10C4&PID_EA60.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA60
%USB\VID_10C4&PID_EA63.DeviceDesc%      =SiLabsDDInstallSection, USB\VID_10C4&PID_EA63
%USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_00
%USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA70&Mi_01
%USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_00
%USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_01
%USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_02
%USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA71&Mi_03
%USB\VID_10C4&PID_EA7A&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_00
%USB\VID_10C4&PID_EA7A&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7A&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_00.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_00
%USB\VID_10C4&PID_EA7B&Mi_01.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_01
%USB\VID_10C4&PID_EA7B&Mi_02.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_02
%USB\VID_10C4&PID_EA7B&Mi_03.DeviceDesc%=SiLabsDDInstallSection, USB\VID_10C4&PID_EA7B&Mi_03


;DDInstall section
[SiLabsDDInstallSection]
AddReg=silabser.AddReg
CopyFiles=Silabser_CopyFiles_FileListSection
FeatureScore=0x40


;DDInstall.Services section
[SiLabsDDInstallSection.Services]
AddService = silabser,0x00000002,silabser.AddService


[silabser.AddService]
DisplayName    = %silabser.SvcDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\silabser.sys

; common registry entries 
[silabser.AddReg]
HKR,,NTMPDriver,,silabser.sys
HKR,,RateLimitPurgeMS, 0x10001, 0x64, 0x00, 0x00, 0x00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,C2,01,00		;115200 initial baud rate
HKR,,InitialLineControl,, "8N1"				;8-bits, No parity, 1 stop bit
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

;DDInstall.HW section
[SiLabsDDInstallSection.HW]
AddReg=SiLabsDDInstallSection.HW.AddReg


[SiLabsDDInstallSection.HW.AddReg]
HKR,,"SelectiveSuspendTimeout",0x00010001,10000
HKR,,"DisableHwAccessInModemStatusIoctls",0x00010001,1
; Attention! The EnablePowerManagewment value is no longer supported.
; To disable Selective Suspend, uncomment the following line:
; HKR,,"DisableS0Idle",0x00010001,1


[Silabser_CopyFiles_FileListSection]
silabser.sys

[SourceDisksNames]
1=%Disk_Description%,"silabser.cat"

[SourceDisksFiles.amd64]
silabser.sys = 1,\x64
[SourceDisksFiles.arm]
silabser.sys = 1,\arm
[SourceDisksFiles.arm64]
silabser.sys = 1,\arm64
[SourceDisksFiles.x86]
silabser.sys = 1,\x86


[DestinationDirs]
Silabser_CopyFiles_FileListSection = 12 ; 13 = Driver package's Driver Store directory (%WINDIR%\System32\DriverStore\FileRepository); 12 = Drivers directory (%SystemRoot%\system32\drivers)) (make sure "ServiceBinary  =" matches usage of 12 vs. 13)


;---------------------------------------------------------------;

[Strings]
; For provider, enter your Company Legal/Offical/Long/Full Name
Provider="Silicon Laboratories Inc."
; For ManufacturerName, enter your Company "Colloquial" Name
ManufacturerName="Silicon Labs"
Disk_Description=                      "Silicon Labs CP210x USB to UART Bridge Installation Disk"
USB\VID_10C4&PID_EA60.DeviceDesc=      "Silicon Labs CP210x USB to UART Bridge"
USB\VID_10C4&PID_EA63.DeviceDesc=      "Silicon Labs CP210x USB to UART Bridge"
USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc="Silicon Labs Dual CP2105 USB to UART Bridge: Enhanced COM Port"
USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc="Silicon Labs Dual CP2105 USB to UART Bridge: Standard COM Port"
USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 0"
USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 1"
USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 2"
USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 3"
USB\VID_10C4&PID_EA7A&Mi_00.DeviceDesc="Silicon Labs Dual CP2105 USB to UART Bridge: Enhanced COM Port"
USB\VID_10C4&PID_EA7A&Mi_01.DeviceDesc="Silicon Labs Dual CP2105 USB to UART Bridge: Standard COM Port"
USB\VID_10C4&PID_EA7B&Mi_00.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 0"
USB\VID_10C4&PID_EA7B&Mi_01.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 1"
USB\VID_10C4&PID_EA7B&Mi_02.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 2"
USB\VID_10C4&PID_EA7B&Mi_03.DeviceDesc="Silicon Labs Quad CP2108 USB to UART Bridge: Interface 3"

silabser.SvcDesc="Silicon Labs CP210x USB to UART Bridge Driver"
